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STACKDOOR RC3
· Description: Security Stacking Shutter System with Independent Certification. 
· Product reference: Stackdoor RC3 Shutter System
· Manufacturer: Charter Global Ltd
· 1 Darwin Close, Reading, Berkshire, RG2 0TB
· Tel: +44 (0) 845 050 8705
· Email: stackdoor@charter-global.com
· Company Certification: ISO 9001
· Product Certifications: BS EN 12604, BS EN 12453
· Product Performance: Product certified to EN1627:2021 burglar resistant security standard

· Arrangement: Top stacking shutter system with no guide rail. Stack-and-pin technology. No head box required. 80% open area to maintain free airflow and visibility. Small stacking zone at high level.
· Opening Sizes: 
· Maximum certified width 6000mm 
· Minimum certified width 760mm
· Maximum certified height 6000mm
· Minimum certified height 2000mm
· Shutter Curtain:
· Material: Steel pins secured into horizontal steel profiles.
· Finish: Standard – Mill finish stainless steel. Option - Horizontal bars (only) may be polyester powder coated to 25 microns. Standard RAL/BS code.
· Frame/Guides: 
· [bookmark: _Hlk158372170]Material: Heavy duty extruded aluminium guide rails anchored directly to the structure. No intermediate guides necessary, smooth and quiet operation with roller guide entry.
· Finish: Standard – Mill finish aluminium. Option - Polyester powder coated to 25 microns. Standard RAL/BS code.
· Bottom Rail:
· Material: Stainless steel.
· Finish: Standard – Brushed stainless steel. Option - Polyester powder coated to 25 microns. Standard RAL/BS code.

· Motor: Standard – Tube motor for low duty cycle or where limited to single phase. Option -External Drive Motor for high duty cycle and larger apertures.






· Operation/Controls: Motorised to allow controlled ascent and descent. Self-locking technology to prevent lifting. Safety on close as assessment directs. Options - Full range of compatible control options available including rotary switch, key switch, remote control and emergency manual crank.

· Installation & Fixing: In accordance with Stackdoor Installation guidelines and recommendations.






All products are based on standard specifications unless otherwise indicated. Options available in blue text.
The large range of options available means bespoke requirements can be accommodated. Please contact the manufacturer to discuss further if the exact product requirement is not covered by this specification.
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