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STACKDOOR ANTI-RAM 
· Description: Security Anti-Ram Grille System with Independent Certification EN1627 RC3. 
· Product reference: Stackdoor Anti-Ram System
· Manufacturer: Charter Global Ltd
· 1 Darwin Close, Reading, Berkshire, RG2 0TB
· Tel: +44 (0) 845 050 8705
· Email: stackdoor@charter-global.com
· Company Certification: ISO 9001
· Product Certifications : BS EN 12604, BS EN 12453, EN1627-30 RC3
· Arrangement: Top stacking grille with anti-ram strengthening system. Stack-and-pin technology. No head box required. 80% open area to maintain free airflow and visibility. 
· Opening Sizes: 
· Maximum width 6000mm
· Minimum height 1500mm
· Shutter Curtain:
· Material: Hardened steel pins secured into horizontal steel profiles. 
· Finish: Standard – Mill finish stainless steel. Option - Horizontal bars (only) may be polyester powder coated to 25 microns. Standard RAL/BS code.
· Frame/Guides: 
· [bookmark: _Hlk158372170]Material: Heavy duty extruded aluminium guide rails with steel reinforcing, anchored directly to the structure. No intermediate guides necessary, smooth and quiet operation with stacking mechanism.
· Finish: Standard – Silver anodised aluminium. Option - Polyester powder coated to 25 microns. Standard RAL/BS code.
· Bottom Rail:
· Material: Stainless steel. 
· Finish: Standard – Brushed stainless steel. Option - Polyester powder coated to 25 microns. Standard RAL/BS code.

· Motor: Standard – Tube motor for low duty cycle or where limited to single phase supply. Option -External Drive Motor for high duty cycle and larger apertures.

· Operation/Controls: Motorised to allow controlled ascent and descent. Self-locking technology to prevent lifting. Safety on close as assessment directs. Options - Full range of compatible control options available including rotary switch, key switch, remote control and emergency manual crank.





· Installation & Fixing: In accordance with Stackdoor Installation guidelines and recommendations.




All products are based on standard specifications unless otherwise indicated. Options available in blue text.
The large range of options available means bespoke requirements can be accommodated. Please contact the manufacturer to discuss further if the exact product requirement is not covered by this specification.
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